The Home coming with A CLASS:

Ethics Assets (P) Ltd Presents

 AUROVILLA

We are pleasure to introduce as Ethics Assets (P) Ltd with decade of expertise in real estate industry in the capital city of Odisha, we are going to present ARTISTHA PREMIUM DUPLEX as AUROVILLA. Its launched with limited 40 unit premium duplex over 2.5 acre of land at the landmark location at RAGHUNATHPUR , besides to ROYAL LAGOON apartment!

Ethics AUROVILLA comes with green environment, modern and spacious designs as well as great service which make you feel the peaceful living experience in our residential units. Each residential unit will come to a home where eco-friendly with affordability. We take care the quality as well as glass clear title so as to give home buyer a trouble free as well as happy ownership.

A world of possibilities beyond living: Home Calling!

Welcome to AUROVILLA, where you will have experiences that go beyond simply living. Immerse yourself in the luxury and comfort that come with ultra-modern amenities, designed to take care of all your needs as well as desires in AUROVILLA enigma!

**SPECIFICATIONS TO BE PROVIDED IN “ETHICS AUROVILLA”**

**STRUCTURE**

STRUCTURE: RCC frame structure with ion filled fly ash brick wall

PLINTH BAND: RCC plinth band will be provided using 16mm, 12mm &

 10mm dia M.S ROD as required & required no of columns as

 per the design specification.

LINTEL: Continuous lintel will be provided at a height of 7” from

 plinth level.

ROOF: RCC roof with water proofing treatment shall be provided at

the height of 10.2” from plinth level as per the required design.

**DOORS, WINDOWS, GRILLS, VENTS & RAILINGS**

FRONT DOORS: Quality teak wood design with Godrej lock, smooth hinges,

 aristocratic premium quality door knob & handle.

DOOR FRAMES: Sal wood except bathrooms & head room

INSIDE DOORS: Decorative finish door, smooth hinges, metallic knob & locks.

BATHROOM DOORS: PVC doors with frames

VENTS: Standard with provision for exhaust fan.

GRILLS: MS Grill with standard design, double coat painting

STAIRCASE RAILING: Stainless STEEL

HEAD ROOM: Iron door with frame

WINDOW: UPVC windows with safety grills

**FLOORING & GRANITE/MARBLE WORKS**
PARKING: Checkered tiles
LOBBY AREAS & STAIRCASE: Granite
INTERNAL FLOORS: 2'X2' Vitrified Tile with skirting on the side
BATHROOM, BALCONY & WET AREA: Anti-skid Ceramic Tiles wall tiling with Dado up

 to 7' height in Bathrooms
KITCHEN AREA: Granite Counter with glazed tiles up to 3ft”

**PLUMBING & FIXTURES**
INTERNAL PIPING: CPVC pipes with provision for washing Machine, Geyser and

 Aqua guard
ETERNAL PIPING: CPVC
BATHROOM, KITCHEN & DINNING FIXTURES (Details of PH WORKS):

 Premium branded fittings (HINDWARE)
DETAILS OF PH WORK : Provision for Washing Machine, wiring for hot and cold
ALTO-SOAP CASE : All Bathrooms and Dinning area Basin
ALTO-TOWEL RAIL: All Bathrooms
HEALTH FAUCET: All Bathrooms
ALTO- TOWEL RING : Dinning Area Basin
MIRRORS: In front of every Basin except in Kitchen
FIXTURES: European pan
Sink: Stainless sink in KITCHEN

**ELECTRICALS**
INTERNAL WIRING: Concealed conduct with copper wiring, adequate outlet for

light, fan, plugs, calling bell & provision for Telephone, TV,

 Internet, Geyser in Bathroom and A/C. Plug points for

 cooking range, Refrigerator, Microwave Ovens,

 Mixer/Grinders in kitchen.

AC POINTS: 3 Nos

TV POINTS: 2 Bedrooms & Drawing

EXTERNAL FIXTURES: Modular Switches of Brand are **HAVELLS/L&T**

**PAINTINGS**
Exterior Cement wash, Acrylic Emulsion Weather Proof Paint (Berger Dulux).

Interior 2 Layer Putty, Primer with 2 Coats Acrylic Emulsion Paint (Berger Dulux).

WATER SUPPLY & DRAINAGE: Individual deep bore well 5” for better water supply & over headwater tank in each duplex, shook pit peptic tank for bathroom & kitchen drainage water.

**MASTER BOUNDARY**: 5 Ft height from the plinth level

**INTERNAL ROAD**: All internal roads will make with INTERBLOCKING BLOCKS.